/**
  ******************************************************************************
  * @file    stm32f4xx_hal_timebase_tim_template.c 
  * @author  MCD Application Team
  * @version V1.4.4
  * @date    22-January-2016
  * @brief   HAL time base based on the hardware TIM Template.
  *    
  *          This file override the native HAL time base functions (defined as weak)
  *          the TIM time base:
  *           + Intializes the TIM peripheral generate a Period elapsed Event each 1ms
  *           + HAL_IncTick is called inside HAL_TIM_PeriodElapsedCallback ie each 1ms
  * 
  ******************************************************************************
  * @attention
  *
  * <h2><center>&copy; COPYRIGHT(c) 2016 STMicroelectronics</center></h2>
  *
  * Redistribution and use in source and binary forms, with or without modification,
  * are permitted provided that the following conditions are met:
  *   1. Redistributions of source code must retain the above copyright notice,
  *      this list of conditions and the following disclaimer.
  *   2. Redistributions in binary form must reproduce the above copyright notice,
  *      this list of conditions and the following disclaimer in the documentation
  *      and/or other materials provided with the distribution.
  *   3. Neither the name of STMicroelectronics nor the names of its contributors
  *      may be used to endorse or promote products derived from this software
  *      without specific prior written permission.
  *
  * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
  * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
  * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
  * DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE
  * FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
  * DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
  * SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER
  * CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY,
  * OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
  * OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
  *
  ******************************************************************************
  */

/* Includes ------------------------------------------------------------------*/
#include "stm32f4xx_hal.h"
#include "stm32f4xx_hal_tim.h"
/** @addtogroup STM32F4xx_HAL_Driver
  * @{
  */

/** @addtogroup HAL_TimeBase
  * @{
  */ 

/* Private typedef -----------------------------------------------------------*/
/* Private define ------------------------------------------------------------*/
/* Private macro -------------------------------------------------------------*/
/* Private variables ---------------------------------------------------------*/
TIM_HandleTypeDef        TimHandle;
/* Private function prototypes -----------------------------------------------*/
void TIM6_DAC_IRQHandler(void);
/* Private functions ---------------------------------------------------------*/

/**
  * @brief  This function configures the TIM6 as a time base source. 
  *         The time source is configured  to have 1ms time base with a dedicated 
  *         Tick interrupt priority. 
  * @note   This function is called  automatically at the beginning of program after
  *         reset by HAL_Init() or at any time when clock is configured, by HAL_RCC_ClockConfig(). 
  * @param  TickPriority: Tick interrupt priority.
  * @retval HAL status
  */
HAL_StatusTypeDef HAL_InitTick (uint32_t TickPriority)
{
  RCC_ClkInitTypeDef    clkconfig;
  uint32_t              uwTimclock, uwAPB1Prescaler = 0U;
  uint32_t              uwPrescalerValue = 0U;
  uint32_t              pFLatency;
  
    /*Configure the TIM6 IRQ priority */
  HAL_NVIC_SetPriority(TIM6_DAC_IRQn, TickPriority ,0U);
  
  /* Enable the TIM6 global Interrupt */
  HAL_NVIC_EnableIRQ(TIM6_DAC_IRQn);
  
  /* Enable TIM6 clock */
  __HAL_RCC_TIM6_CLK_ENABLE();
  
  /* Get clock configuration */
  HAL_RCC_GetClockConfig(&clkconfig, &pFLatency);
  
  /* Get APB1 prescaler */
  uwAPB1Prescaler = clkconfig.APB1CLKDivider;
  
  /* Compute TIM6 clock */
  if (uwAPB1Prescaler == RCC_HCLK_DIV1) 
  {
    uwTimclock = HAL_RCC_GetPCLK1Freq();
  }
  else
  {
    uwTimclock = 2*HAL_RCC_GetPCLK1Freq();
  }
  
  /* Compute the prescaler value to have TIM6 counter clock equal to 1MHz */
  uwPrescalerValue = (uint32_t) ((uwTimclock / 1000000U) - 1U);
  
  /* Initialize TIM6 */
  TimHandle.Instance = TIM6;
  
  /* Initialize TIMx peripheral as follow:
  + Period = [(TIM6CLK/1000) - 1]. to have a (1/1000) s time base.
  + Prescaler = (uwTimclock/1000000 - 1) to have a 1MHz counter clock.
  + ClockDivision = 0
  + Counter direction = Up
  */
  TimHandle.Init.Period = (1000000U / 1000U) - 1U;
  TimHandle.Init.Prescaler = uwPrescalerValue;
  TimHandle.Init.ClockDivision = 0;
  TimHandle.Init.CounterMode = TIM_COUNTERMODE_UP;
  if(HAL_TIM_Base_Init(&TimHandle) == HAL_OK)
  {
    /* Start the TIM time Base generation in interrupt mode */
    return HAL_TIM_Base_Start_IT(&TimHandle);
  }
  
  /* Return function status */
  return HAL_ERROR;
}

/**
  * @brief  Suspend Tick increment.
  * @note   Disable the tick increment by disabling TIM6 update interrupt.
  * @param  None
  * @retval None
  */
void HAL_SuspendTick(void)
{
  /* Disable TIM6 update Interrupt */
  __HAL_TIM_DISABLE_IT(&TimHandle, TIM_IT_UPDATE);
}

/**
  * @brief  Resume Tick increment.
  * @note   Enable the tick increment by Enabling TIM6 update interrupt.
  * @param  None
  * @retval None
  */
void HAL_ResumeTick(void)
{
  /* Enable TIM6 Update interrupt */
  __HAL_TIM_ENABLE_IT(&TimHandle, TIM_IT_UPDATE);
}

/**
  * @brief  Period elapsed callback in non blocking mode
  * @note   This function is called  when TIM6 interrupt took place, inside
  * HAL_TIM_IRQHandler(). It makes a direct call to HAL_IncTick() to increment
  * a global variable "uwTick" used as application time base.
  * @param  htim : TIM handle
  * @retval None
  */
void HAL_TIM_PeriodElapsedCallback(TIM_HandleTypeDef *htim)
{
  HAL_IncTick();
}

/**
  * @brief  This function handles TIM interrupt request.
  * @param  None
  * @retval None
  */
void TIM6_DAC_IRQHandler(void)
{
  HAL_TIM_IRQHandler(&TimHandle);
}

/**
  * @}
  */ 

/**
  * @}
  */ 

/************************ (C) COPYRIGHT STMicroelectronics *****END OF FILE****/
