\section{Bootloader}
For the first released hardware sample of moray ruby 2 for the WCA side the
bootloader v1.0.0.0 has to be used. The release is available
\href{http://dabsvn01.internal.novero.com/svn/0\_31X\_P0513\_moray\_ruby2/trunk/development/software/releases/wca/bootloader/20151127\_1.0.0.0/wca\_bootloader\_R262144.elf.p.S}{here}.\\
The flash procedure has changed slightly. Because we don't have any longer
the $TEL\_ON$ signal now the bootloader stays in bootloader mode for $t=2s$
after switching on WCA. Within that period the bootloader accepts the
connect request of the pc-side flash tool. If that period expires without
receiving the connect request the bootloader will start the WCA application.
\section{Hardware modification}
To connect the WCA's Debug interface you have to populate 2 wires (Rx, Tx)
between WCA's Debug interface and RS232 level shifter.\\
On WCA side the $UART\_RX$ has to be connected to free pad of resistor
$R35$. $UART_\_TX$ has to be connected to free pad of resistor $R21$. For details see figure\ref{fig:photo} and \ref{fig:schematic}.
\begin{figure}[htb]
\includegraphics[scale=0.16, angle=90]{IMG_20151130_095112.eps}
\caption{Assembled WCA Debug Interface}
\label{fig:photo}
\end{figure}
\begin{figure}[htb]
\includegraphics[scale=0.7,angle=270]{populate.eps}
\caption{Schematic populating details}
\label{fig:schematic}
\end{figure}

